Procedure:

1. Cylinder must be rotated to be upritght
2. Cylinder must be translated to 0,0,
3. Range of angles are changed from [180,180] to [0, 360]
4. Extract profile
5. Calculate mean and Ra
6. Re order points and save them to textfiles
7. Open textfile, proceed as usual